##### Dialup service

Dialup service properties window contains the following pages:

- Main (standard, see above).
- Service parameters is similar to the same page in Periodic service. In addition, contains the following elements:

- Pool name is the name of the pool to issue the addresses from. If the pool is registered in UTM5, the first available IP address from it is issued. Otherwise the pool name itself is passed instead.
  This parameter is cached by UTM5 RADIUS.

- Maximum timeout is the maximum session duration until forced break (in seconds).

- Limit of simultaneous sessions sets the maximum number of concurrent connections that may be established with the same login.
  This parameter is cached by UTM5 RADIUS.

- Login prefix is the prefix to be prepended automatically to the user’s login on creation of a service link.
- Dynamic IP address allocation is used to link this service to another one of IP traffic type (also having this flag set) in order to perform combined tariffication based together on connection time and traffic consumption. One account may have only one hotspot or dialup service with this flag set.

- Price per hour contains the list of connection time prices for various time ranges. Must contain at least one entry. Time is counted with precision to seconds.
- RADIUS parameters .

Parameters of the corresponding service link are described in Dialup service link.