##### Hotspot service

Hotspot service properties window contains the following pages:

- Main (standard, Pressing opens the service properties window focused on the Main page. This page includes the following elements:).
- Service parameters is similar to the same page in Periodic service. In addition, contains the following elements:

- Limit of simultaneous sessions sets the maximum number of concurrent connections that may be established with the same login.
- Dynamic IP address allocation is used to link this service to another one of IP traffic type (also having this flag set) in order to perform combined tariffication based together on connection time and traffic consumption. One account may have only one hotspot or dialup service with this flag set.

- Allowed networks contains the list of allowed IP addresses from which the user is allowed to authorize on the UTM5 web interface. Authorization requests from other addresses are denied.
- RADIUS parameters .
- Price per hour contains the list of connection time prices for various time ranges.

Parameters of the corresponding service link are described in Hotspot service link.